**Alto Shaam Cook & Hold Smoker BBQ Program Specifications for RFP**

**ITEM 1: DOUBLE STACK COOK AND HOLD SMOKER UNIT**

COOK HOLD OVEN CABINET SMOKER, ELECTRIC Two (2) Required

Dimensions: 33.38(h) x 25.7(w) x 33.5(d)

Cook Hold & Smoker Oven, electric, low temperature, 100 lb. capacity - (9) 12" x 20" x 2-1/2" full-size pans, simple or deluxe controls, programmable recipes, probe, includes (1) sample bag each of cherry, hickory, apple & maple wood chips, heavy-duty stainless steel exterior with solid door, stainless steel wire shelves, 1 rib rack, 3-1/2" casters (2 rigid, 2 swivel with brakes), EcoSmart®, cULus, UL EPH Classified, CE, IPX4, EAC, TUV NORD, N11942

2 ea 120v/60/1-ph, 17.0 amps, 2.0 kW, NO cord, NO plug

2 ea Deluxe Controls – Touch screen user interface with customizable home screen, programmable recipes, unlimited cook stages, recipe management, service diagnostics, and reporting on screen; enables access to ChefLinc™ remote oven management system to monitor ovens, view reports and push/pull recipes and oven settings via Wi-Fi or Ethernet connectivity

1 ea 2 Single point probes (DELUXE ONLY)

2 ea Window door, hinged on right

2 ea Stainless steel exterior, standard

2 ea Wood Chips, Cherry, 2.55 cu. ft., reference weight 40 lb. bulk pack

2 ea Wood Chips, Apple, 2.55 cu. ft., reference weight 40 lb. bulk pack

2 ea Wood Chips, Maple, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 ea Wood Chips, Hickory, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 ea Stacking Kit C&H, for stacking one cook hold smoker oven on top of another like unit

1 ea Caster Package, 5"

2 cs Non-Caustic cleaner, (6) 32 oz bottles

2 ea Drip Pan, with drain, stainless steel, 1-11/16" (43mm)

Approved Manufacturer: Alto Shaam

Scope of work for DOUBLE STACK Alto-Shaam Cook & Hold Smoker Units:

* K-12 ISD:
  + Provide adequate space for new unit, including disconnect and relocate any existing equipment in designated space
  + Provide two (2) 120 Volt, 1 phase, 20 amp dedicated receptacles
  + Provide cord & plug, and final electrical connection, per oven cavity
* Awarded Kitchen Equipment Contractor:
  + Receive new Alto-Shaam Cook & Hold Smokers
  + Deliver new Cook & Hold Smoker to designated campus(es)
  + Installation including:  uncrate, set in place, peel all protective plastic, stack, add casters, and make ready for final electrical connection(s) by others, per the manufacturer guidelines
  + Discard of all crating materials, trash & debris from the campus in a proper trash receptacle
* Successful Awarded Manufacturer’s Rep Group:
  + Provide a thorough training on operation, safety, cleaning, and simple preventative maintenance
  + Upload all Alto-Shaam K-12 Smoker Cook & Hold BBQ Recipes

**ITEM 2: SINGLE STACK COOK AND HOLD SMOKER UNIT ON CASTERS**

COOK HOLD OVEN CABINET SMOKER, ELECTRIC (1 REQ'D)

Dimensions: 33.38(h) x 25.7(w) x 33.5(d)

Cook Hold & Smoker Oven, electric, low temperature, 100 lb. capacity - (9) 12" x 20" x 2-1/2" full-size pans, simple or deluxe controls, programmable recipes, probe, includes (1) sample bag each of cherry, hickory, apple & maple wood chips, heavy-duty stainless steel exterior with solid door, stainless steel wire shelves, 1 rib rack, 3-1/2" casters (2 rigid, 2 swivel with brakes), EcoSmart®, cULus, UL EPH Classified, CE, IPX4, EAC, TUV NORD, N11942

1 ea 120v/60/1-ph, 17.0 amps, 2.0 kW, NO cord, NO plug

1 ea Deluxe Controls – Touch screen user interface with customizable home screen, programmable recipes, unlimited cook stages, recipe management, service diagnostics, and reporting on screen; enables access to ChefLinc™ remote oven management system to monitor ovens, view reports and push/pull recipes and oven settings via Wi-Fi or Ethernet connectivity

1 ea 2 Single point probes (DELUXE ONLY)

1 ea Solid door, hinged on right, standard

1 ea Stainless steel exterior, standard

1 ea Extended Drip Tray, for C&H 750/1750 Series

1 ea Wood Chips, Cherry, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 ea Wood Chips, Apple, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 ea Wood Chips, Maple, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 ea Wood Chips, Hickory, 2.55 cu. ft., reference weight 40 lb. bulk pack

1 cs Non-Caustic cleaner, (6) 32 oz bottles

1 ea Caster Package, 5”

Approved Manufacturer: Alto Shaam

Scope of work for DOUBLE STACK Alto-Shaam Cook & Hold Smoker Units:

* K-12 ISD:
  + Provide adequate space for new unit, including disconnect and relocate any existing equipment in designated space
  + Provide one (1) 120 Volt, 1 phase, 20 amp dedicated receptacles
  + Provide cord & plug, and final electrical connection, per oven cavity
* Awarded Kitchen Equipment Contractor:
  + Receive new Alto-Shaam Cook & Hold Smoker
  + Deliver new Cook & Hold Smoker to designated campus(es)
  + Installation including:  uncrate, set in place, peel all protective plastic, level, and make ready for final electrical connection(s) by others, per the manufacturer guidelines
  + Discard of all crating materials, trash & debris from the campus in a proper trash receptacle
* Successful Awarded Manufacturer’s Rep Group:
  + Provide a thorough training on operation, safety, cleaning, and simple preventative maintenance
  + Upload all Alto-Shaam K-12 Smoker Cook & Hold BBQ Recipes

Alto Shaam Cook and Hold Smoker BBQ Program - Suggest Supplementary Items

ITEM 1 - HI-TEMP FOOD PAN (6 REQ'D)

Cambro Model 24LPHP110

H-Pan™ High Heat Hot Food Pan, 1/2 size long, 4" deep, hi-temp plastic, -40°F to 375°F, non-stick surface, won't bend or dent, black, NSF

ITEM 2 - PLATTER (4 REQ'D)

American Metalcraft Model SQP10 Dimensions: 1.38(h) x 12(w) x 12(d)

Endurance™ Platter, 12" sq. x 1-3/8"H, small, break-resistant, melamine, white

ITEM 3 - FOOD PAN (6 REQ'D)

Cambro Model 24LPCW110

Camwear® Food Pan, 5.3 qt. capacity, 4" deep, 1/2 size long, polycarbonate, black, NSF

6 ea 2 year warranty

ITEM 4 - HI-TEMP FOOD PAN (6 REQ'D)

Cambro Model 24LPHP110

H-Pan™ High Heat Hot Food Pan, 1/2 size long, 4" deep, hi-temp plastic, -40°F to 375°F, non-stick surface, won't bend or dent, black, NSF

ITEM 5 - PORTION CONTROL SPOON / LADLE (6 REQ'D)

American Metalcraft Model SPN4

Spooner, 4 oz., 3-3/8" diameter solid stainless steel bowl, ladle style, 10-3/4" bakelite grip handle, 1-piece, green

ITEM 6 - UTILITY TONGS (6 REQ'D)

American Metalcraft Model UT1200 Dimensions: 12(w)

Utility Tongs, 12" long, .7mm stainless, tempered flat steel spring, standard weight

ITEM 7 - PORTION CONTROL SPOON / LADLE (6 REQ'D)

American Metalcraft Model SPNP4

Spooner, 4 oz., 3-3/8" diameter perforated stainless steel bowl, ladle style, 10-3/4" bakelite grip handle, 1-piece, green

ITEM 8 - DISPOSABLE CONTAINER MEAL KIT (4 REQ'D)

American Metalcraft Model TV9 Dimensions: 10.4(h) x 9(w) x 9(d)

Canvas Bag, 9" dia. x 10-3/8" H, Pre-shrunk, machine washable, reusable, cream, canvas

ITEM 9 - PLATTER (2 REQ'D)

American Metalcraft Model MEL23 Dimensions: 2(h) x 18(w) x 8.25(d)

Endurance™ Platter, 18"L x 8-1/4"W x 2"H, rectangular, melamine, white, (dishwasher safe up to 200 degrees)

ITEM 10 - BOWL (2 REQ'D)

American Metalcraft Model MELSL82 Dimensions: 5(h) x 8(w)

Endurance™ Serving Bowl, 40 oz., 8" dia. x 5"H, slanted, round, break-resistant, dishwasher safe, melamine, white

ITEM 11 - BOWL (2 REQ'D)

American Metalcraft Model MELSL112 Dimensions: 6.5(h) x 12(w)

Endurance™ Serving Bowl, 112 oz., 12" dia. x 6-1/2"H, slanted, round, break-resistant, dishwasher safe, melamine, white

ITEM 12 - BIB APRON (1 REQ'D)

Mercer Culinary Model M63206DEN Dimensions: 29.75(w) x 34(d)

Scout Bib Apron, 29-3/4" x 34", extra-long adjustable straps in pocketed seams, large 2-section pocket, 3-section pencil pocket, contrasting stitching, cross-hatch sateen fabric, 65/35 poly cotton blend, charcoal gray